(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A3")
  (title_block
    (title "Multirotor wiring diagram")
    (rev "v0.1")
  )
  (layers
    (0 "F.Cu" power)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" power)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (49 "F.Fab" user)
    (50 "User.1" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "Purple") (material "Direct Printing"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "prepreg") (thickness 0.1) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "core") (thickness 1.24) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "prepreg") (thickness 0.1) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x0000000_7ffffff9)
      (plot_on_all_layers_selection 0x706f0f0_80000007)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 5)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "wiring_diagram")
    )
  )
  (net 0 "")
  (footprint "Library:PDB" (layer "F.Cu")
    (at 151.4 149.48 90)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0 90) (layer "F.SilkS") hide)
    (fp_text_box "VCC	GND"
    (start 4.5 -24.5) (end 0 -17) (angle 270) (layer "F.Mask")    )
    (fp_text_box "VCC	GND"
    (start 29.75 -27) (end 34.25 -34.5) (angle 90) (layer "F.Mask")    )
    (fp_text_box "VCC	GND"
    (start 4.5 -35) (end 0 -27.5) (angle 270) (layer "F.Mask")    )
    (fp_text_box "5V GND"
    (start 7 -11.5) (end 14.5 -8) (layer "F.Mask")    )
    (fp_text_box "VCC	GND"
    (start 5.5 -12.5) (end 1 -5) (angle 270) (layer "F.Mask")    )
    (fp_text_box "VCC	GND"
    (start 29 -3) (end 33.5 -10.5) (angle 90) (layer "F.Mask")    )
    (fp_text_box "VCC	GND"
    (start 30.5 -15.5) (end 35 -23) (angle 90) (layer "F.Mask")    )
    (pad "1" thru_hole circle (at 13 -46 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 21 -46 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 9 -9 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 11 -9 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "5" thru_hole circle (at 16 -9 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "6" thru_hole circle (at 18 -9 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "7" thru_hole circle (at 33 -32 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 33 -30 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "9" thru_hole circle (at 33 -21 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "10" thru_hole circle (at 33 -18 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "13" thru_hole circle (at 32 -8 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "14" thru_hole circle (at 32 -6 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "15" thru_hole circle (at 2 -33 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "16" thru_hole circle (at 2 -29 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "17" thru_hole circle (at 2 -23 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "18" thru_hole circle (at 2 -19 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "19" thru_hole circle (at 2.5 -10.5 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "20" thru_hole circle (at 2.5 -7.5 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:reciever" (layer "F.Cu")
    (at 231.88 225.4 180)
    (fp_text reference "REF**" (at 0 -0.5 180 unlocked) (layer "F.SilkS"))
    (fp_text value "Reciever" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (fp_text_box "S V G"
    (start 17.5 -6) (end 1 0) (angle 270) (layer "F.Mask")    )
    (pad "1" thru_hole circle (at 2.5 -5 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 4.5 -5 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 6.5 -5 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 8.5 -5 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 10.5 -5 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 12.5 -5 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 14.5 -5 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 2.5 -3 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 4.5 -3 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 6.5 -3 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 8.5 -3 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 10.5 -3 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 12.5 -3 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 14.5 -3 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 2.5 -1 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 4.5 -1 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 6.5 -1 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 8.5 -1 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 10.5 -1 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 12.5 -1 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 14.5 -1 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:servo" (layer "F.Cu")
    (at 305.62 172.72 90)
    (fp_text reference "REF**" (at 0 -0.5 90 unlocked) (layer "F.SilkS"))
    (fp_text value "servo" (at 0 1 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90 unlocked) (layer "F.Fab"))
    (fp_text_box "sig	5V GND"
    (start 16.5 -0.75) (end 21 -11.25) (angle 90) (layer "F.Mask")    )
    (pad "1" thru_hole circle (at 20 -9.5 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 20 -6 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 20 -2.5 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:soldered" (layer "F.Cu")
    (at 262.255 140.97)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "soldered" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "5v" (at 8.382 -15.24 unlocked) (layer "F.SilkS"))
    (fp_text user "GND" (at 7.62 -12.7 unlocked) (layer "F.SilkS"))
    (fp_text user "SCL SDA" (at 48.26 -7.62 unlocked) (layer "F.SilkS"))
    (fp_text user "5V   GND  CLK  MISO MOSI CS" (at 63.5 -7.62 unlocked) (layer "F.SilkS"))
    (fp_text user "Servo 1" (at 5.08 -5.08 unlocked) (layer "F.SilkS"))
    (fp_text user "Servo 3" (at 30.48 -5.08 unlocked) (layer "F.SilkS"))
    (fp_text user "Servo 2" (at 17.78 -5.08 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 12.7 -7.62) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 7.62 -2.54) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 10.16 -2.54) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 12.7 -2.54) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "5" thru_hole circle (at 5.08 -12.7) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "6" thru_hole circle (at 5.08 -15.24) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "7" thru_hole circle (at 20.32 -2.54) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 22.86 -2.54) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "9" thru_hole circle (at 25.4 -2.54) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "10" thru_hole circle (at 25.4 -7.62) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "11" thru_hole circle (at 17.78 -15.24) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "12" thru_hole circle (at 17.78 -12.7) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "13" thru_hole circle (at 30.48 -12.7) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "14" thru_hole circle (at 30.48 -15.24) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "15" thru_hole circle (at 33.02 -2.54) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "16" thru_hole circle (at 35.56 -2.54) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "17" thru_hole circle (at 38.1 -2.54) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "18" thru_hole circle (at 38.1 -7.62) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "19" thru_hole circle (at 43.18 -15.24) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "20" thru_hole circle (at 43.18 -12.7) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "21" thru_hole circle (at 53.34 -15.24) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "22" thru_hole circle (at 53.34 -12.7) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "23" thru_hole circle (at 50.8 -10.16) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "24" thru_hole circle (at 55.88 -10.16) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "25" thru_hole circle (at 55.88 -5.08) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "26" thru_hole circle (at 50.8 -5.08) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "27" thru_hole circle (at 78.74 -5.08) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "28" thru_hole circle (at 86.36 -5.08) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "29" thru_hole circle (at 91.44 -5.08) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "30" thru_hole circle (at 96.52 -5.08) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "31" thru_hole circle (at 78.74 -10.16) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "32" thru_hole circle (at 86.36 -10.16) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "33" thru_hole circle (at 91.44 -10.16) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "34" thru_hole circle (at 96.52 -10.16) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "35" thru_hole circle (at 96.52 -15.24) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "36" thru_hole circle (at 96.52 -12.7) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "37" thru_hole circle (at 71.12 -10.16) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "38" thru_hole circle (at 63.5 -10.16) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:flight controller" (layer "F.Cu")
    (at 191.2 207.24)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "flight controller" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "7" thru_hole rect (at 5.25 -20.75) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "7" thru_hole rect (at 5.25 -18.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "7" thru_hole rect (at 5.25 -16.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "7" thru_hole rect (at 5.25 -14.25) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "7" thru_hole rect (at 5.25 -12) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "7" thru_hole rect (at 5.25 -9.75) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "7" thru_hole rect (at 12 -1.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 3.25 -20.75) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 3.25 -18.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 3.25 -16.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 3.25 -14.25) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 3.25 -12) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 3.25 -9.75) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 10 -1.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "9" thru_hole circle (at 1 -20.75) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "9" thru_hole circle (at 1 -18.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "9" thru_hole circle (at 1 -16.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "9" thru_hole circle (at 1 -14.25) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "9" thru_hole circle (at 1 -12) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "9" thru_hole circle (at 1 -9.75) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "9" thru_hole circle (at 7.75 -1.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "11" thru_hole circle (at 14 -1.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "12" thru_hole circle (at 16.25 -1.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "13" thru_hole circle (at 18.5 -1.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "15" thru_hole circle (at 20.75 -1.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "16" thru_hole circle (at 23.25 -1.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "17" thru_hole circle (at 25.5 -1.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "18" thru_hole circle (at 27.5 -1.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "20" thru_hole circle (at 29.5 -1.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:servo" (layer "F.Cu")
    (at 290.38 172.72 90)
    (fp_text reference "REF**" (at 0 -0.5 90 unlocked) (layer "F.SilkS"))
    (fp_text value "servo" (at 0 1 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90 unlocked) (layer "F.Fab"))
    (fp_text_box "sig	5V GND"
    (start 16.5 -0.75) (end 21 -11.25) (angle 90) (layer "F.Mask")    )
    (pad "1" thru_hole circle (at 20 -9.5 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 20 -6 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 20 -2.5 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:servo" (layer "F.Cu")
    (at 275.14 172.72 90)
    (fp_text reference "REF**" (at 0 -0.5 90 unlocked) (layer "F.SilkS"))
    (fp_text value "servo" (at 0 1 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90 unlocked) (layer "F.Fab"))
    (fp_text_box "sig	5V GND"
    (start 16.5 -0.75) (end 21 -11.25) (angle 90) (layer "F.Mask")    )
    (pad "1" thru_hole circle (at 20 -9.5 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 20 -6 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 20 -2.5 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MPU 6050" (layer "F.Cu")
    (at 345.545 94.32)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "MPU 6050" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (fp_text_box "V G SC SD INT"
    (start 1.75 -4) (end 16.33 -0.5) (layer "F.Mask")    )
    (pad "1" thru_hole circle (at 3.5 -1.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 5.5 -1.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 7.5 -1.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 9.5 -1.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "5" thru_hole circle (at 11.5 -1.5) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:SD breakout board" (layer "F.Cu")
    (at 368.735 105.0973 180)
    (fp_text reference "REF**" (at 0 -0.5 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "SD breakout board" (at 0 -30 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -31.5 180 unlocked) (layer "F.Fab"))
    (fp_text_box "CD\n\nCS\n\nDI\n\nDO\n\nCLK\n\nGND\n\n3v\n\n5v"
    (start -24.25 -22) (end -0.75 -29.0254) (angle 90) (layer "F.Mask")    )
    (pad "6" thru_hole circle (at -2.5 -27 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "7" thru_hole circle (at -5 -27 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at -7.5 -27 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "9" thru_hole circle (at -10 -27 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "10" thru_hole circle (at -12.5 -27 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "11" thru_hole circle (at -15 -27 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "12" thru_hole circle (at -17.5 -27 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "13" thru_hole circle (at -20 -27 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "14" thru_hole circle (at -22.5 -27 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:ESC" (layer "B.Cu")
    (at 147.77 81.5 -90)
    (fp_text reference "REF**" (at 0 0.5 90 unlocked) (layer "B.SilkS"))
    (fp_text value "ESC" (at 0 -1 90 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90 unlocked) (layer "B.Fab"))
    (fp_text_box "GND  sig"
    (start 4 4) (end 11.5 0) (angle 180) (layer "B.Mask")    )
    (fp_text_box "Motor connections"
    (start 15 20) (end 0 26.5) (layer "B.Mask")    )
    (fp_text_box "GND"
    (start 11.5 4) (end 15 0) (angle 180) (layer "B.Mask")    )
    (fp_text_box "Vbatt"
    (start 0 4) (end 4 0) (angle 180) (layer "B.Mask")    )
    (pad "1" thru_hole circle (at 1.5 1.5 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 13 1.5 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 6.5 1.5 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 8.5 1.5 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "5" thru_hole circle (at 2.5 25 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "7" thru_hole circle (at 6.5 25 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 10.5 25 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Module:Arduino_UNO_R3" (layer "B.Cu")
    (at 292.735 31.75 180)
    (descr "Arduino UNO R3, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino UNO R3")
    (attr through_hole)
    (fp_text reference "REF**" (at 1.27 3.81) (layer "B.SilkS"))
    (fp_text value "Arduino_UNO_R3" (at 0 -22.86) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -20.32) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "5" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "6" thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "7" thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole oval (at 17.78 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "9" thru_hole oval (at 22.86 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "10" thru_hole oval (at 25.4 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "11" thru_hole oval (at 27.94 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "12" thru_hole oval (at 30.48 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "13" thru_hole oval (at 33.02 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "14" thru_hole oval (at 35.56 0 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "15" thru_hole oval (at 35.56 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "16" thru_hole oval (at 33.02 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "17" thru_hole oval (at 30.48 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "18" thru_hole oval (at 27.94 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "19" thru_hole oval (at 25.4 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "20" thru_hole oval (at 22.86 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "21" thru_hole oval (at 20.32 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "22" thru_hole oval (at 17.78 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "23" thru_hole oval (at 13.72 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "24" thru_hole oval (at 11.18 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "25" thru_hole oval (at 8.64 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "26" thru_hole oval (at 6.1 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "27" thru_hole oval (at 3.56 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "28" thru_hole oval (at 1.02 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "29" thru_hole oval (at -1.52 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "30" thru_hole oval (at -4.06 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "31" thru_hole oval (at -6.6 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "32" thru_hole oval (at -9.14 -48.26 90) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Module.3dshapes/Arduino_UNO_R3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:ESC" (layer "B.Cu")
    (at 147.77 63.72 -90)
    (fp_text reference "REF**" (at 0 0.5 90 unlocked) (layer "B.SilkS"))
    (fp_text value "ESC" (at 0 -1 90 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90 unlocked) (layer "B.Fab"))
    (fp_text_box "GND  sig"
    (start 4 4) (end 11.5 0) (angle 180) (layer "B.Mask")    )
    (fp_text_box "Vbatt"
    (start 0 4) (end 4 0) (angle 180) (layer "B.Mask")    )
    (fp_text_box "GND"
    (start 11.5 4) (end 15 0) (angle 180) (layer "B.Mask")    )
    (fp_text_box "Motor connections"
    (start 15 20) (end 0 26.5) (layer "B.Mask")    )
    (pad "1" thru_hole circle (at 1.5 1.5 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 13 1.5 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 6.5 1.5 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 8.5 1.5 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "5" thru_hole circle (at 2.5 25 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "7" thru_hole circle (at 6.5 25 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 10.5 25 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:ESC" (layer "B.Cu")
    (at 147.77 45.94 -90)
    (fp_text reference "REF**" (at 0 0.5 90 unlocked) (layer "B.SilkS"))
    (fp_text value "ESC" (at 0 -1 90 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90 unlocked) (layer "B.Fab"))
    (fp_text_box "GND  sig"
    (start 4 4) (end 11.5 0) (angle 180) (layer "B.Mask")    )
    (fp_text_box "Vbatt"
    (start 0 4) (end 4 0) (angle 180) (layer "B.Mask")    )
    (fp_text_box "GND"
    (start 11.5 4) (end 15 0) (angle 180) (layer "B.Mask")    )
    (fp_text_box "Motor connections"
    (start 15 20) (end 0 26.5) (layer "B.Mask")    )
    (pad "1" thru_hole circle (at 1.5 1.5 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 13 1.5 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 6.5 1.5 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 8.5 1.5 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "5" thru_hole circle (at 2.5 25 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "7" thru_hole circle (at 6.5 25 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 10.5 25 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:ESC" (layer "B.Cu")
    (at 147.32 28.38 -90)
    (fp_text reference "REF**" (at 0 0.5 90 unlocked) (layer "B.SilkS"))
    (fp_text value "ESC" (at 0 -1 90 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90 unlocked) (layer "B.Fab"))
    (fp_text_box "GND  sig"
    (start 4 4) (end 11.5 0) (angle 180) (layer "B.Mask")    )
    (fp_text_box "Vbatt"
    (start 0 4) (end 4 0) (angle 180) (layer "B.Mask")    )
    (fp_text_box "Motor connections"
    (start 15 20) (end 0 26.5) (layer "B.Mask")    )
    (fp_text_box "GND"
    (start 11.5 4) (end 15 0) (angle 180) (layer "B.Mask")    )
    (pad "1" thru_hole circle (at 1.5 1.5 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 13 1.5 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 6.5 1.5 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 8.5 1.5 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "5" thru_hole circle (at 2.5 25 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "7" thru_hole circle (at 6.5 25 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 10.5 25 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
  )
)
